

**HSB750**

**LED Magic Beam light**

Power Supply: AC100-240V;50Hz-60Hz

Light Source: 2x15W RGBW( 4 in 1) Tianxin LED

Power Consumption: 35W

Controls: DMX512;Sound activation,Auto,Master/slave

DMX Channels: 10 Channels

Life time: 60000 hours

Flash: Flash speed up to 20 times/sec Control panel: 4 LCD tube + 4 press bottom DMX connector: 2×Rj45 input and output; 2×XLR input and output

Dimmer: 0-100% linearly adjustable

Protection rate: IP20

Working environment: up to 40°C

Material: ﬁre-proof ABS plastic, White housing.

Dimension size: 187×170x276mm Packing size: 270×270×350mm 560×560×385mm (4pcs/ctn) N.W: 1.5kg

G.W: 2.2kg /11.2kg (4pcs/ctn)

NIGHTSUN PROFESSIONAL LIGHTING PROVIDER.